<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="23.8" y2="0" width="0" layer="20"/>
<wire x1="23.8" y1="0" x2="23.8" y2="21.58" width="0" layer="20"/>
<wire x1="23.8" y1="21.58" x2="0" y2="21.58" width="0" layer="20"/>
<wire x1="0" y1="21.58" x2="0" y2="0" width="0" layer="20"/>
<text>VCC</text>
<text>VOUT</text>
<text>GND</text>
</plain>
<libraries>
<library name="capacitor-wima">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C2.5-3">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 5 x 3 mm, grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TC26V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="0204/5">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 5 mm</description>
</package>
<package name="TO92-EBC-OVAL">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="con-headers-jp">
<description>&lt;b&gt;Male(J), Female(P) and Pin Headers&lt;/b&gt;&lt;p&gt;Version 1.02 - 03/10/2009&lt;p&gt;
This library is a collection of various pin headers and AMP, Molex and 3M board-to-board connectors. 
This library assumes the notion of JACKS(male) and PLUGS(female) as represented by the J and P symbols.
Standard male/female pin header types are available in common 0.1" and 2 mm pitch types with alternate mirrored footprints as well.
&lt;p&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;
USE AT YOUR OWN RISK!&lt;p&gt;
&lt;author&gt;Copyright (C) 2008, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;&lt;/author&gt;</description>
<packages>
<package name="SIP-100-03-40">
<description>&lt;b&gt;SIP Header&lt;/b&gt; - 0.1", 40 mil drill</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="capacitor-wima" package="C2.5-3" value=""/>
<element name="C2" library="capacitor-wima" package="C2.5-3" value=""/>
<element name="Q3" library="crystal" package="TC26V" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="R5" library="adafruit" package="0204/5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="0204/5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="adafruit" package="0204/5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="0204/5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="adafruit" package="TO92-EBC-OVAL" value="2N2222">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P1" library="con-headers-jp" package="SIP-100-03-40" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="R6" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="Q3" pad="1"/>
<contactref element="P1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="R5" pad="1"/>
<contactref element="T1" pad="C"/>
</signal>
<signal name="N$5">
<contactref element="T1" pad="B"/>
<contactref element="C2" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="Q3" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="R1" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="P1" pad="1"/>
</signal>
<signal name="VOUT">
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="T1" pad="E"/>
<contactref element="R6" pad="2"/>
<contactref element="P1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
