<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="38.786" y2="0" width="0" layer="20"/>
<wire x1="38.786" y1="0" x2="38.786" y2="22.85" width="0" layer="20"/>
<wire x1="38.786" y1="22.85" x2="0" y2="22.85" width="0" layer="20"/>
<wire x1="0" y1="22.85" x2="0" y2="0" width="0" layer="20"/>
<text>TX</text>
<text>RX</text>
<text>GND</text>
<text>3V3</text>
<text>PWR</text>
<text>VCC</text>
<hole x="2.54" y="21.59" drill="1.2"/>
<hole x="2.54" y="1.27" drill="1.2"/>
<hole x="34.29" y="21.59" drill="1.2"/>
<hole x="34.29" y="1.27" drill="1.2"/>
</plain>
<libraries>
<library name="rcl">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="wirepad">
<packages>
<package name="SMD1,27-2,54">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="RN41">
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X07">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="GeekAmmo">
<description>&lt;h3&gt;GeekAmmo  Library&lt;/h3&gt;

These are parts used by the GeekAmmo company (now part of SparkFun Electronics)!

 If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="rcl" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl" package="C0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X07" value="">
<attribute name="VALUE"/>
</element>
<element name="FACTORY_RST" library="wirepad" package="SMD1,27-2,54" value="WIREPADSMD1,27-254">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun" package="RN41" value="BLUETOOTH-RN41&quot;"/>
<element name="STATUS" library="led" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T3" library="SparkFun-PowerIC" package="SOT23-3" value="LM3480IM4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T2" library="GeekAmmo" package="SOT23-3" value="N-MOSFET">
<attribute name="DATASHEET" value="http://www.fairchildsemi.com/ds/BS/BSS138.pdf"/>
<attribute name="URL" value="http://au.element14.com/fairchild-semiconductor/bss138/mosfet-n-ch-50v-220ma-sot-23/dp/2323154"/>
<attribute name="ELEMENT14" value="2323154"/>
<attribute name="OTHER" value=""/>
<attribute name="DIGIKEY" value="BSS138TR-ND"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="rcl" package="R0603" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="R0603" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="GeekAmmo" package="SOT23-3" value="N-MOSFET">
<attribute name="DATASHEET" value="http://www.onsemi.com/pub/Collateral/NTR4501N-D.PDF"/>
<attribute name="URL" value="http://au.element14.com/fairchild-semiconductor/bss138/mosfet-n-ch-50v-220ma-sot-23/dp/2323154"/>
<attribute name="ELEMENT14" value="2323154"/>
<attribute name="OTHER" value=""/>
<attribute name="DIGIKEY" value="BSS138TR-ND"/>
<attribute name="NAME"/>
</element>
<element name="R4" library="rcl" package="R0603" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R0603" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CONN" library="led" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="MASTER" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POWER" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AUTODISCOVERY" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BAUD" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ5" library="jumper" package="SJ" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$1" pad="12"/>
<contactref element="U$1" pad="28"/>
<contactref element="U$1" pad="29"/>
<contactref element="T3" pad="3"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="CONN" pad="C"/>
<contactref element="L3" pad="C"/>
<contactref element="J1" pad="3"/>
<contactref element="POWER" pad="2"/>
</signal>
<signal name="TX">
<contactref element="U$1" pad="14"/>
<contactref element="T1" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="RX">
<contactref element="U$1" pad="13"/>
<contactref element="T2" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="U$1" pad="5"/>
<contactref element="POWER" pad="1"/>
</signal>
<signal name="STATUS">
<contactref element="U$1" pad="19"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="STATUS" pad="C"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="21"/>
</signal>
<signal name="FACTORY_RST">
<contactref element="FACTORY_RST" pad="1"/>
<contactref element="U$1" pad="22"/>
</signal>
<signal name="RTS">
<contactref element="U$1" pad="15"/>
<contactref element="SJ5" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="T3" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="3V3">
<contactref element="J1" pad="7"/>
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="11"/>
<contactref element="STATUS" pad="A"/>
<contactref element="C3" pad="1"/>
<contactref element="T3" pad="1"/>
<contactref element="T2" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="T1" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="MASTER" pad="2"/>
<contactref element="AUTODISCOVERY" pad="2"/>
<contactref element="BAUD" pad="2"/>
</signal>
<signal name="TXH">
<contactref element="J1" pad="5"/>
<contactref element="T1" pad="3"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="RXH">
<contactref element="J1" pad="6"/>
<contactref element="T2" pad="3"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R6" pad="2"/>
<contactref element="CONN" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="R7" pad="1"/>
<contactref element="L3" pad="A"/>
</signal>
<signal name="AUTODISCOVERY">
<contactref element="U$1" pad="20"/>
<contactref element="AUTODISCOVERY" pad="1"/>
</signal>
<signal name="CTS">
<contactref element="U$1" pad="16"/>
<contactref element="SJ5" pad="2"/>
</signal>
<signal name="BT_MASTER">
<contactref element="U$1" pad="3"/>
<contactref element="MASTER" pad="1"/>
</signal>
<signal name="BD_RATE">
<contactref element="U$1" pad="4"/>
<contactref element="BAUD" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
